




1. Run “Kyocera setup” file




1. Click on “Accept”




1. Custom install – Add custom device – Kyocera task alfa 1801




1. Click on “Add port”




1. Click on “Next tab”



1. Give the ip address 10.101.10.54 and click on next tab.




1. Click on Finish tab





1. For Job Accounting


Go to the printer propertis



2. “Device setting “=> ”Administrator” follow the step mention in snap



After that use below setting in client tool.



1. For Page setup

